<div class="content"><p>The <b>IPBOOTP_IF_STATS</b> structure is an MIB entry,
stores per interface statistics for the IPBOOTP. All of the IP addresses are in
network order. This structure is read-only.</p><dl>
<dd>
<div><pre> typedef struct _IPBOOTP_IF_STATS {
   DWORD IS_State;
   DWORD IS_SendFailures;
   DWORD IS_ReceiveFailures;
   DWORD IS_ArpUpdateFailures;
   DWORD IS_RequestsReceived;
   DWORD IS_RequestsDiscarded;
   DWORD IS_RepliesReceived;
   DWORD IS_RepliesDiscarded;
 } IPBOOTP_IF_STATS,
  *PIPBOOTP_IF_STATS;
</pre></div>
</dd></dl><p><b>IS_State: </b>Contains status of the IPBOOTP. This
member is read-only.</p><dl>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Value</p>
   </th>
   <th>
   <p>Meaning</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>IPBOOTP_STATE_ENABLED</p>
  <p>0x00000001</p>
  </td>
  <td>
  <p>The interface is enabled.</p>
  </td>
 </tr><tr>
  <td>
  <p>IPBOOTP_STATE_BOUND</p>
  <p>0x00000002</p>
  </td>
  <td>
  <p>The socket is bound and can listen to the IPBOOTP
  packets <a href="https://go.microsoft.com/fwlink/?LinkId=90281" data-linktype="external">[RFC1542]</a>.</p>
  </td>
 </tr></tbody></table>
</dd></dl><p><b>IS_SendFailures: </b>The number of relay messages
that could not be sent.</p><p><b>IS_ReceiveFailures: </b>The number of times errors
were encountered in receiving relay messages.</p><p><b>IS_ArpUpdateFailures: </b>The number of times
errors were encountered while updating the ARP cache.</p><p><b>IS_RequestsReceived: </b>The number of IP BOOTP
requests received.</p><p><b>IS_RequestsDiscarded: </b>The number of IP BOOTP
requests discarded.</p><p><b>IS_RepliesReceived: </b>The number of IP BOOTP
replies received.</p><p><b>IS_RepliesDiscarded: </b>The number of IP BOOTP
replies discarded.</p></div>