<div class="content"><p>The <b>RASI_CONNECTION_3</b> structure contains information
for a connection, including the GUID that identifies the connection, the <a href="fc2dfae9-0d04-4e1d-97c9-c51c2dc06c3b#gt_f30fdc41-d7c1-422e-b5a8-9dcce071ebeb" data-linktype="relative-path">Network Access Protection (NAP)</a>,
and the PPP-related data for the connection.</p><dl>
<dd>
<div><pre> typedef struct _RASI_CONNECTION_3 {
   DWORD dwVersion;
   DWORD dwSize;
   DWORD dwConnection;
   WCHAR wszUserName[257];
   ROUTER_INTERFACE_TYPE dwInterfaceType;
   GUID guid;
   PPP_INFO_3 PppInfo3;
   RAS_QUARANTINE_STATE rasQuarState;
   FILETIME timer;
 } RASI_CONNECTION_3,
  *PRASI_CONNECTION_3;
</pre></div>
</dd></dl><p><b>dwVersion: </b>Determines the version of the <b>RASI_CONNECTION_3</b>
structure used.</p><p><b>dwSize: </b>This SHOULD be set to 0. This MAY be
used to specify the size, in bytes, of this<b> RASI_CONNECTION_3</b> structure.</p><p><b>dwConnection: </b>Contains the connection handle
that specifies a unique identifier of a connection.</p><p><b>wszUserName: </b>Specifies a null-terminated
Unicode string that contains the name of the user on this connection.</p><p><b>dwInterfaceType: </b>A <b>ROUTER_INTERFACE_TYPE</b>
(section <a href="849c1f9e-9d6f-4408-840e-ee9ae253ae01" data-linktype="relative-path">2.2.1.1.1</a>)
value that specifies the type of interface.</p><p><b>guid: </b>Specifies a GUID that identifies the
connection. For an incoming connection, this GUID is valid only as long as the
connection is active.</p><p><b>PppInfo3: </b>Specifies a <b>PPP_INFO_3</b>
(section <a href="b76fc63b-1288-4f8a-a14b-410193fc6602" data-linktype="relative-path">2.2.1.2.74</a>)
structure<a id="Appendix_A_Target_60"></a><a aria-label="Product behavior note 60" href="3bb906f0-b077-47ab-ad11-d8d807afde26#Appendix_A_60" data-linktype="relative-path">&lt;60&gt;</a> that contains information about
the PPP negotiation for this connection.</p><p><b>rasQuarState: </b>Specifies the NAP quarantine
state for the connection through the <b>RAS_QUARANTINE_STATE</b> (section <a href="4393ed23-2164-4283-8198-e704da2664f4" data-linktype="relative-path">2.2.1.1.3</a>)<span><span> </span></span>that
contains the quarantine state of this connection.</p><p><b>timer: </b>Specifies the NAP probation time for
the connection in the UTC. This value is valid only if the <b>rasQuarState</b>
has a value of RAS_QUAR_STATE_PROBATION (see <b>RAS_QUARANTINE_STATE </b>section
2.2.1.1.3).</p></div>