<div class="content"><p> </p><p>The <b>FAX_EVENT_DEVICE_STATUS</b> structure defines
information about the status of a fax device. This structure is embedded in the
<b>FAX_EVENT_EX</b> (section <span><a href="3a9ae7f7-9825-43cd-aa78-1c077fd99bd2" data-linktype="relative-path">2.2.67</a></span>) and <b>FAX_EVENT_EX_1</b> (section
<span><a href="425c3686-00b8-493d-bba5-d4ce677e47db" data-linktype="relative-path">2.2.68</a></span>)
structures as a union field.</p><p>This data structure is custom marshaled as follows and uses
the custom-marshaling rules defined in section <span><a href="a660ed3e-062f-4b49-ab5b-0ba19ea7598d" data-linktype="relative-path">2.2.1</a></span>.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p>Fixed_Portion</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
</tbody></table><p><b>Fixed_Portion (8 bytes):</b></p><dl>
<dd>
<table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p>dwDeviceId</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>dwNewStatus</p>
  </td>
 </tr>
</tbody></table>
</dd>
<dd>
<p><b>dwDeviceId (4 bytes): </b>A
<b>DWORD</b> (<span><a href="../ms-dtyp/cca27429-5689-4a16-b2b4-9325d93e4ba2" data-linktype="relative-path">[MS-DTYP]</a></span>
section <span><a href="../ms-dtyp/262627d8-3418-4627-9218-4ffe110850b2" data-linktype="relative-path">2.2.9</a></span>)
value indicating the identification number of the device that had a status
change.</p>
</dd>
<dd>
<p><b>dwNewStatus (4 bytes): </b>A
<b>DWORD</b> value indicating the new status. The value is a combination of
values from <b>FAX_ENUM_DEVICE_STATUS</b> (section <span><a href="267364f2-e9ba-460c-a4b4-10faf8fc8920" data-linktype="relative-path">2.2.64</a></span>).</p>
</dd></dl></div>