<div class="content"><p> </p><p>The <b>FAX_AddOutboundGroup (Opnum 51)</b> method is called
by the client to add a new outbound <span><a href="46aba9c4-ebb1-4b10-86ac-4bb3025657b9#gt_20b15ad8-82b1-47ef-a494-561c9cdee7fa" data-linktype="relative-path">routing group</a></span>.</p><p>In response, the server MUST check for the client&#39;s <b>fax
user account</b> access to write <span><a href="46aba9c4-ebb1-4b10-86ac-4bb3025657b9#gt_826f969a-1e12-40f8-9e81-784b0a84a295" data-linktype="relative-path">outbound groups</a></span>. The
server MUST check for duplicate group names in a case-insensitive manner. On
success, the server MUST add a new outbound routing group to the fax server.
Devices can be added to a newly created group by using <b>FAX_SetOutboundGroup</b>
(section <span><a href="c72ba43e-75c3-4171-bb7a-70e8161b10c4" data-linktype="relative-path">3.1.4.1.85</a></span>).<a id="Appendix_A_Target_67"></a><a aria-label="Product behavior note 67" href="056171e7-80bc-45ff-8107-66ba3abb2023#Appendix_A_67" data-linktype="relative-path">&lt;67&gt;</a></p><dl>
<dd>
<div><pre> error_status_t FAX_AddOutboundGroup(
   [in] handle_t hFaxHandle,
   [in, string, ref] LPCWSTR lpwstrGroupName
 );
</pre></div>
</dd></dl><p><b>hFaxHandle: </b>The RPC binding handle for this
call. The client SHOULD reuse the RPC binding handle used as an input <i>hBinding</i>
argument for the <b>FAX_ConnectFaxServer</b> (section <span><a href="5cbfd38d-7a14-4560-ad24-9ed78f19a3bb" data-linktype="relative-path">3.1.4.1.10</a></span>) or <b>FAX_ConnectionRefCount</b>
(section 3.1.4.1.11) method call used to connect to the fax server.</p><p><b>lpwstrGroupName: </b>A pointer to a
null-terminated character string that uniquely identifies a new group name.
This value cannot be <b>NULL</b>. The group name is expected to be
case-insensitive.</p><p><b>Return Values: </b>This method MUST return
0x00000000 (ERROR_SUCCESS) for success; otherwise, it MUST return one of the
following error codes, one of the fax-specific errors that are defined in
section <span><a href="cbe6c4fb-4dda-4f6c-9701-0d490ba0d105" data-linktype="relative-path">2.2.52</a></span>, or one of
the other standard errors defined in <span><a href="../ms-erref/1bc92ddf-b79e-413c-bbaa-99a5281a6c90" data-linktype="relative-path">[MS-ERREF]</a></span>
section <span><a href="../ms-erref/18d8fbe8-a967-4f1c-ae50-99ca8e491d2d" data-linktype="relative-path">2.2</a></span>.</p><dl>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Return value/code</p>
   </th>
   <th>
   <p>Description</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>ERROR_ACCESS_DENIED</p>
  <p>0x00000005</p>
  </td>
  <td>
  <p>Access is denied. The client&#39;s fax user account does
  not have the FAX_ACCESS_MANAGE_CONFIG access rights.</p>
  </td>
 </tr><tr>
  <td>
  <p>ERROR_DUP_NAME</p>
  <p>0x00000034</p>
  </td>
  <td>
  <p>The group name specified by the <i>lpwstrGroupName</i>
  parameter is &#34;&lt; All devices&gt;&#34;.</p>
  </td>
 </tr><tr>
  <td>
  <p>ERROR_INVALID_PARAMETER</p>
  <p>0x00000057</p>
  </td>
  <td>
  <p>The fax server tried to return
  FAX_ERR_NOT_SUPPORTED_ON_THIS_SKU, but the client fax API version
  FAX_API_VERSION_0 (described in section 3.1.4.1.10) does not support this
  error code.</p>
  </td>
 </tr><tr>
  <td>
  <p>ERROR_BUFFER_OVERFLOW</p>
  <p>0x0000006F</p>
  </td>
  <td>
  <p>The length of the character string specified by the <i>lpwstrGroupName</i>
  parameter, excluding the length of the terminating null terminator, is equal
  to or greater than 128 characters.</p>
  </td>
 </tr><tr>
  <td>
  <p>ERROR_REGISTRY_CORRUPT</p>
  <p>0x000003F7</p>
  </td>
  <td>
  <p>The fax server cannot store the new outbound routing
  group configuration in the <span><a href="46aba9c4-ebb1-4b10-86ac-4bb3025657b9#gt_2d67ea57-10e6-422f-985e-694834945a02" data-linktype="relative-path">registry</a></span>. The
  registry could be corrupted.</p>
  </td>
 </tr><tr>
  <td>
  <p>FAX_ERR_NOT_SUPPORTED_ON_THIS_SKU</p>
  <p>0x00001B63</p>
  </td>
  <td>
  <p>The fax client module API version (described in
  section 3.1.4.1.10) is FAX_API_VERSION_1 or above, and the fax server is
  running on a version of the operating system that does not support the
  requested operation.<a id="Appendix_A_Target_68"></a><a aria-label="Product behavior note 68" href="056171e7-80bc-45ff-8107-66ba3abb2023#Appendix_A_68" data-linktype="relative-path">&lt;68&gt;</a></p>
  </td>
 </tr></tbody></table>
</dd></dl><p><b>Exceptions Thrown: </b>No exceptions are thrown
except those by the underlying <span><a href="46aba9c4-ebb1-4b10-86ac-4bb3025657b9#gt_8a7f6700-8311-45bc-af10-82e10accd331" data-linktype="relative-path">RPC</a></span> protocol <span><a href="../ms-rpce/290c38b1-92fe-4229-91e6-4fc376610c15" data-linktype="relative-path">[MS-RPCE]</a></span>. 
</p></div>