<div class="content"><p>The BlindTransfer packet is transmitted from a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_60e0e1fa-66fe-41e1-b5e3-ceab97e53506" data-linktype="relative-path">client</a> to a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_434b0234-e970-4e8c-bdfa-e16a30d96703" data-linktype="relative-path">server</a> in a <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_8a7f6700-8311-45bc-af10-82e10accd331" data-linktype="relative-path">remote procedure call</a>.
Sending this packet performs a blind or single-step transfer of the specified
call to the specified destination address.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Req_Func</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved1</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwRequestID</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">hCall</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">lpszDestAddress</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwCountryCode</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved2</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved3</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved4</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved5</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved6</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved7</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved8</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved9</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved10</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">VarData
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">...</p>
  </td>
 </tr>
</tbody></table><p><b>Req_Func (4 bytes): </b>An unsigned 32-bit
integer. The identifier of the function that will be invoked on the remote
server. This value MUST be set to 8. </p><dl>
<dd>
<p><b>Return Values</b></p>
</dd>
<dd>
<p>On completion of <a href="c28c36d0-579b-4e20-a100-f4e71012d5f8" data-linktype="relative-path">ClientRequest</a>, this field
contains the result of the encapsulated telephony request. A nonzero request ID
value indicates that the request is in progress and will complete
asynchronously. A <a href="e0e8af90-24f1-4dbc-8d4e-01b8e4e7cb53" data-linktype="relative-path">LINEERR_Constants</a>
value indicates synchronous failure.</p>
</dd>
<dd>
<p>Returns a positive request identifier if the
function will be completed asynchronously or a negative error number if an
error occurs. The dwParam2 parameter of the corresponding <a href="8f5bc349-fd55-46f2-b0bc-dc9f757317a9" data-linktype="relative-path">LINE_REPLY</a> packet is zero
if the function succeeds, or it is a negative error number if an error occurs.
If the client specified a nonzero value in the dwRequestID field of the packet,
the same value MUST be used for the returned positive request identifier. </p>
</dd>
<dd>
<p>The following table shows the return values for this
function. </p>
</dd>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Value</p>
   </th>
   <th>
   <p>Meaning</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>LINEERR_INVALCALLHANDLE</p>
  <p>0x80000018</p>
  </td>
  <td>
  <p>The handle to the call is invalid.</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_NOMEM</p>
  <p>0x80000044</p>
  </td>
  <td>
  <p>Not enough memory is available.</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_INVALCALLSTATE</p>
  <p>0x8000001C</p>
  </td>
  <td>
  <p>The call state is invalid.</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONFAILED</p>
  <p>0x80000048</p>
  </td>
  <td>
  <p>The operation failed.</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_ADDRESSBLOCKED</p>
  <p>0x80000053</p>
  </td>
  <td>
  <p>The address is blocked.</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_RESOURCEUNAVAIL</p>
  <p>0x8000004B</p>
  </td>
  <td>
  <p>The resource is unavailable.</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_INVALCOUNTRYCODE</p>
  <p>0x80000022</p>
  </td>
  <td>
  <p>The country/region code is invalid.</p>
  </td>
 </tr></tbody></table>
</dd></dl><p><b>Reserved1 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>dwRequestID (4 bytes): </b>An unsigned 32-bit
integer. The identifier of the asynchronous request.</p><p><b>hCall (4 bytes): </b>An <a href="7f4089a0-7432-4ef0-8eeb-5aafe407c07e" data-linktype="relative-path">HCALL</a>. The handle to the
call to be transferred. One way in which the client can obtain a valid hCall is
from the <a href="0a8905e3-647f-4e98-aca8-2fa77eedb2e7" data-linktype="relative-path">LINE_CALLSTATE</a>
packet sent by the remote server. The application MUST be an owner of this
call. The call state of hCall must be connected. For hCall to be in connected
state, the client needs to send an <a href="1076f351-bdb9-4a83-844c-811a729d7228" data-linktype="relative-path">Answer</a> packet to the
remote server.</p><p><b>lpszDestAddress (4 bytes): </b>An unsigned 32-bit
integer. The offset, in bytes, in the VarData field of a null-terminated
Unicode string that identifies where to transfer the call.</p><p><b>dwCountryCode (4 bytes): </b>An unsigned 32-bit
integer. The country code of the destination. The implementation SHOULD use
this field to select the call progress protocols for the destination address.
If a value of 0 is specified, the service provider SHOULD use a default. TAPI
does not validate dwCountryCode when this function is called.</p><p><b>Reserved2 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved3 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved4 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved5 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved6 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved7 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved8 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved9 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved10 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>VarData (variable): </b>Contains a null-terminated
Unicode string that is indicated in the lpszDestAddress field.</p><dl>
<dd>
<p>The contents of this field MUST be DWORD-aligned, as
specified in <a href="../ms-dtyp/cca27429-5689-4a16-b2b4-9325d93e4ba2" data-linktype="relative-path">[MS-DTYP]</a>
section <a href="../ms-dtyp/262627d8-3418-4627-9218-4ffe110850b2" data-linktype="relative-path">2.2.9</a>.</p>
</dd></dl></div>