<div class="content"><p>The GetAddressID packet is transmitted from a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_60e0e1fa-66fe-41e1-b5e3-ceab97e53506" data-linktype="relative-path">client</a> to a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_434b0234-e970-4e8c-bdfa-e16a30d96703" data-linktype="relative-path">server</a> in a <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_8a7f6700-8311-45bc-af10-82e10accd331" data-linktype="relative-path">remote procedure call</a>.
Sending this packet returns the address identifier that is associated with
address, in a different format on the specified line.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Req_Func</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved1</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">hLine</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">lpdwAddressID</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwAddressMode</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">lpsAddress</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwSize</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved2</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved3</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved4</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved5</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved6</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved7</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved8</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved9</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">VarData
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">...</p>
  </td>
 </tr>
</tbody></table><p><b>Req_Func (4 bytes): </b>An unsigned 32-bit
integer. The identifier of the function that will be invoked on the remote
server. This value MUST be set to 22.</p><dl>
<dd>
<p><b>Return Values</b></p>
</dd>
<dd>
<p>On completion of <a href="c28c36d0-579b-4e20-a100-f4e71012d5f8" data-linktype="relative-path">ClientRequest</a>, this field
contains the result of the encapsulated telephony request. A value of 0
indicates success, and a <a href="e0e8af90-24f1-4dbc-8d4e-01b8e4e7cb53" data-linktype="relative-path">LINEERR_Constants</a>
value indicates failure. The remote server MUST complete this call
synchronously.</p>
</dd>
<dd>
<p>MUST return zero if the function succeeds or an
error number if an error occurs. Common return values are as follows:</p>
</dd>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Name</p>
   </th>
   <th>
   <p>Value</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>LINEERR_INVALLINEHANDLE</p>
  </td>
  <td>
  <p>0x8000002B</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONUNAVAIL</p>
  </td>
  <td>
  <p>0x80000049</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_INVALADDRESS</p>
  </td>
  <td>
  <p>0x80000010</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONFAILED</p>
  </td>
  <td>
  <p>0x80000048</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_NOMEM</p>
  </td>
  <td>
  <p>0x80000044</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_RESOURCEUNAVAIL</p>
  </td>
  <td>
  <p>0x8000004B</p>
  </td>
 </tr></tbody></table>
</dd></dl><p><b>Reserved1 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>hLine (4 bytes): </b>An HLINE. The handle to the
line whose address is to be retrieved. This field MUST have been obtained by
sending the <a href="2759c744-e040-4c5d-b4b5-215d391f0490" data-linktype="relative-path">Open</a>
packet.</p><p><b>lpdwAddressID (4 bytes): </b>An unsigned 32-bit
integer. Set to TAPI_NO_DATA (0xFFFFFFFF). Upon successful completion of the
request, this field contains the address identifier.</p><p><b>dwAddressMode (4 bytes): </b>An unsigned 32-bit
integer. The address mode of the address that is contained in lpsAddress. <a href="fa130dd9-e33e-4f7e-8274-574ae8c622d3" data-linktype="relative-path">LINEADDRESSMODE_DIALABLEADDR</a>
MUST be specified for the dwAddressMode parameter. </p><p><b>lpsAddress (4 bytes): </b>An unsigned 32-bit
integer. The offset, in bytes, in the VarData field of a packet that holds the
address that is assigned to the specified line device. The format of the
address is determined by the dwAddressMode parameter.</p><p><b>dwSize (4 bytes): </b>An unsigned 32-bit integer. The
size of the address that is contained in lpsAddress. The size of the string
MUST include the null terminator.</p><p><b>Reserved2 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved3 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved4 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved5 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved6 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved7 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved8 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved9 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>VarData (variable): </b>Present on successful
completion of the request. Contains a packet that holds the address that is
assigned to the specified line device, as indicated in the lpsAddress field.</p><dl>
<dd>
<p>The contents of this field MUST be DWORD-aligned, as
specified in <a href="../ms-dtyp/cca27429-5689-4a16-b2b4-9325d93e4ba2" data-linktype="relative-path">[MS-DTYP]</a>
section <a href="../ms-dtyp/262627d8-3418-4627-9218-4ffe110850b2" data-linktype="relative-path">2.2.9</a>.</p>
</dd></dl></div>