<div class="content"><p>The <b>MIB_IPNETROW</b> structure contains information for
an Address Resolution Protocol (ARP) table entry for an IPv4 address. This
structure is used in <b>MIB_OPAQUE_INFO</b> (section <a href="169e435d-a975-4c1c-bf41-55fd2bd76125" data-linktype="relative-path">2.2.1.2.52</a>) structure.</p><dl>
<dd>
<div><pre> typedef struct _MIB_IPNETROW {
   DWORD dwIndex;
   DWORD dwPhysAddrLen;
   BYTE bPhysAddr[8];
   DWORD dwAddr;
   DWORD dwType;
 } MIB_IPNETROW,
  *PMIB_IPNETROW;
</pre></div>
</dd></dl><p><b>dwIndex: </b>This MUST be the interface index of
an adapter.</p><p><b>dwPhysAddrLen: </b>The length, in bytes, of the
physical address.</p><p><b>bPhysAddr: </b>The physical address.</p><p><b>dwAddr: </b>The IPv4 address.</p><p><b>dwType: </b>The type of ARP entry. This type MUST
be one of the following values.</p><dl>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Value</p>
   </th>
   <th>
   <p>Meaning</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>0x00000001</p>
  </td>
  <td>
  <p>Other</p>
  </td>
 </tr><tr>
  <td>
  <p>0x00000002</p>
  </td>
  <td>
  <p>Invalid</p>
  </td>
 </tr><tr>
  <td>
  <p>0x00000003</p>
  </td>
  <td>
  <p>Dynamic</p>
  </td>
 </tr><tr>
  <td>
  <p>0x00000004</p>
  </td>
  <td>
  <p>Static</p>
  </td>
 </tr></tbody></table>
</dd></dl><p> </p></div>