<div class="content"><p>The <b>IPPREFIX</b> structure contains an IP address and the
prefix length of its associated network.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p>Endpoint
  (128 bytes)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>PrefixLength</p>
  </td>
 </tr>
</tbody></table><p><b>Endpoint (128 bytes): </b>MUST be laid out as a
sockaddr_in or sockaddr_in6 structure as specified in <a href="https://go.microsoft.com/fwlink/?LinkId=90367" data-linktype="external">[RFC2553]</a>. The
remaining bytes SHOULD be set to 0x00.</p><p><b>PrefixLength (4 bytes): </b>The prefix length of
the associated network of the IP address in <b>Endpoint</b>.</p></div>