<div class="content"><p>The MonitorDigits packet is transmitted from a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_60e0e1fa-66fe-41e1-b5e3-ceab97e53506" data-linktype="relative-path">client</a> to a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_434b0234-e970-4e8c-bdfa-e16a30d96703" data-linktype="relative-path">server</a> in a <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_8a7f6700-8311-45bc-af10-82e10accd331" data-linktype="relative-path">remote procedure call</a>.
Sending this packet enables or disables the unbuffered detection of digits that
are received on the call. Each time a digit of the specified digit modes is
detected, a <a href="ee945d1b-6b97-40e2-abd8-02b5b790c47f" data-linktype="relative-path">LINE_MONITORDIGITS</a>
packet is sent to the application by TAPI, indicating which digit is detected.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Req_Func</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved1</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">hCall</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwDigitModes</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved2</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved3</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved4</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved5</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved6</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved7</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved8</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved9</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved10</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved11</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved12</p>
  </td>
 </tr>
</tbody></table><p><b>Req_Func (4 bytes): </b>An unsigned 32-bit
integer. The identifier of the function that will be invoked on the remote
server. This value MUST be set to 49.</p><dl>
<dd>
<p><b>Return Values</b></p>
</dd>
<dd>
<p>On completion of <a href="c28c36d0-579b-4e20-a100-f4e71012d5f8" data-linktype="relative-path">ClientRequest</a>, this field
contains the result of the encapsulated telephony request. A value of 0
indicates success, and a <a href="e0e8af90-24f1-4dbc-8d4e-01b8e4e7cb53" data-linktype="relative-path">LINEERR_Constants</a>
value indicates failure. The remote server MUST complete this call
synchronously.</p>
</dd>
<dd>
<p>MUST return zero if the function succeeds or an
error number if an error occurs. Common return values are as follows: </p>
</dd>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Name</p>
   </th>
   <th>
   <p>Value</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>LINEERR_INVALCALLHANDLE</p>
  </td>
  <td>
  <p>0x80000018</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONUNAVAIL</p>
  </td>
  <td>
  <p>0x80000049</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_INVALCALLSTATE</p>
  </td>
  <td>
  <p>0x8000001C</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONFAILED</p>
  </td>
  <td>
  <p>0x80000048</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_INVALDIGITMODE</p>
  </td>
  <td>
  <p>0x80000027</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_RESOURCEUNAVAIL</p>
  </td>
  <td>
  <p>0x8000004B</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_NOMEM</p>
  </td>
  <td>
  <p>0x80000044</p>
  </td>
 </tr></tbody></table>
</dd></dl><p><b>Reserved1 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>hCall (4 bytes): </b>An <a href="7f4089a0-7432-4ef0-8eeb-5aafe407c07e" data-linktype="relative-path">HCALL</a>. The handle to the
call on which digits are to be detected. The call state of hCall can be any
state except idle or disconnected. One way of obtaining a valid hCall is by
sending the <a href="c9acdfde-22de-43ff-b491-23a9ed72fb31" data-linktype="relative-path">MakeCall</a>
packet. Also a valid hCall can be obtained from <a href="0a8905e3-647f-4e98-aca8-2fa77eedb2e7" data-linktype="relative-path">LINE_CALLSTATE</a> packet sent
by the remote server.</p><p><b>dwDigitModes (4 bytes): </b>An unsigned 32-bit
integer. The digit modes that are to be monitored. A dwDigitModes parameter
with a value of 0 cancels digit monitoring. The dwDigitModes parameter MUST
have one of the <a href="fec875c7-afff-494a-94d1-b9d6fe292d5f" data-linktype="relative-path">LINEDIGITMODE_Constants</a>.</p><p><b>Reserved2 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved3 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved4 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved5 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved6 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved7 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved8 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved9 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved10 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved11 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved12 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p></div>