<div class="content"><p>The <b>IPRIP_PEER_STATS</b> structure is an MIB entry that
describes the statistics kept about neighboring routers. All IP addresses are
in network order. This structure is read-only. This structure is used in <a href="45250002-d774-4bc2-ab2e-6992341b5f45" data-linktype="relative-path"><b>IPRIP_MIB_GET_INPUT_DATA (section 2.2.1.2.161)</b></a>
and <a href="4fc16996-6de7-4f99-8cea-40e1f42931e1" data-linktype="relative-path"><b>IPRIP_MIB_GET_OUTPUT_DATA (section 2.2.1.2.162)</b></a>
structures.  </p><dl>
<dd>
<div><pre> typedef struct _IPRIP_PEER_STATS {
   DWORD PS_LastPeerRouteTag;
   DWORD PS_LastPeerUpdateTickCount;
   DWORD PS_LastPeerUpdateVersion;
   DWORD PS_BadResponsePacketsFromPeer;
   DWORD PS_BadResponseEntriesFromPeer;
 } IPRIP_PEER_STATS,
  *PIPRIP_PEER_STATS;
</pre></div>
</dd></dl><p><b>PS_LastPeerRouteTag: </b>The route tag last
received from the peer.</p><p><b>PS_LastPeerUpdateTickCount: </b>The number of
updates received from peer.</p><p><b>PS_LastPeerUpdateVersion: </b>The RIP version of
the last update received from peer.</p><p><b>PS_BadResponsePacketsFromPeer: </b>The number of
bad response packets received from peer.</p><p><b>PS_BadResponseEntriesFromPeer: </b>The number of
bad entries in responses received from peer.</p></div>