<div class="content"><p>The <b>RAS_DEVICE_INFO</b> structure contains device
information.</p><dl>
<dd>
<div><pre> typedef struct _RAS_DEVICE_INFO {
   DWORD dwVersion;
   BOOL fWrite;
   BOOL fRasEnabled;
   BOOL fRouterEnabled;
   BOOL fRouterOutboundEnabled;
   DWORD dwTapiLineId;
   DWORD dwError;
   DWORD dwNumEndPoints;
   DWORD dwMaxOutCalls;
   DWORD dwMaxInCalls;
   DWORD dwMinWanEndPoints;
   DWORD dwMaxWanEndPoints;
   RASDEVICETYPE eDeviceType;
   GUID guidDevice;
   CHAR szPortName[17];
   CHAR szDeviceName[129];
   WCHAR wszDeviceName[129];
 } RAS_DEVICE_INFO,
  *PRAS_DEVICE_INFO;
</pre></div>
</dd></dl><p><b>dwVersion: </b>Specifies the version of the Rasrpc
server.<a id="Appendix_A_Target_155"></a><a aria-label="Product behavior note 155" href="3bb906f0-b077-47ab-ad11-d8d807afde26#Appendix_A_155" data-linktype="relative-path">&lt;155&gt;</a></p><p><b>fWrite: </b>If set to 1, specifies that device
information needs to be stored on RRAS. If set to 0, specifies that the device
information does not need to be stored.</p><p><b>fRasEnabled: </b>If set to 1, specifies that the
device is enabled for incoming connections. If set to 0, specifies that the
device is not enabled for incoming connections.</p><p><b>fRouterEnabled: </b>If set to 1, specifies that
the device is enabled for both incoming and outgoing demand-dial connection. If
set to 0, specifies that the device is not enabled for both incoming and
outgoing demand-dial connection.</p><p><b>fRouterOutboundEnabled: </b>If set to 1, specifies
that the device is enabled for outgoing Demand dial connection. This can be set
to 1 only when <b>fRouterEnabled</b> is set to 0.<a id="Appendix_A_Target_156"></a><a aria-label="Product behavior note 156" href="3bb906f0-b077-47ab-ad11-d8d807afde26#Appendix_A_156" data-linktype="relative-path">&lt;156&gt;</a></p><p><b>dwTapiLineId: </b>Unique <b>TAPI</b> identifier
for the device.</p><p><b>dwError: </b>Specifies the return status as
explained in section <a href="c39d153e-2f97-4e11-8aff-bcf983869dc9" data-linktype="relative-path">2.2.1.2.218</a>
for the <b>retcode</b> field. </p><p><b>dwNumEndPoints: </b>Specifies the number of WAN
end points available for the device.</p><p><b>dwMaxOutCalls: </b>Specifies the maximum number of
outgoing connections allowed on the device.</p><p><b>dwMaxInCalls: </b>Specifies the maximum number of
incoming connections allowed on the device.</p><p><b>dwMinWanEndPoints: </b>Specifies the minimum
number of WAN <b>end points</b> allowed on the device.</p><p><b>dwMaxWanEndPoints: </b>Specifies the maximum
number of WAN <b>end points</b> allowed on the device.</p><p><b>eDeviceType: </b>Specifies the <b>RASDEVICETYPE</b>
enumeration type.</p><p><b>guidDevice: </b>A <b>GUID</b> uniquely identifying
the device. This value MUST NOT be used when eDeviceType is RDT_Modem.</p><p><b>szPortName: </b>Specifies a null-terminated ASCII
string specifying the Port Name.</p><p><b>szDeviceName: </b>Specifies a null-terminated
ASCII string specifying the Device Name.</p><p><b>wszDeviceName: </b>SHOULD<a id="Appendix_A_Target_157"></a><a aria-label="Product behavior note 157" href="3bb906f0-b077-47ab-ad11-d8d807afde26#Appendix_A_157" data-linktype="relative-path">&lt;157&gt;</a> contain a null-terminated
Unicode string specifying the Device Name.<span> </span></p></div>