<div class="content"><p>The SetDefaultMediaDetection packet is transmitted from a
TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_60e0e1fa-66fe-41e1-b5e3-ceab97e53506" data-linktype="relative-path">client</a> to a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_434b0234-e970-4e8c-bdfa-e16a30d96703" data-linktype="relative-path">server</a> in a <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_8a7f6700-8311-45bc-af10-82e10accd331" data-linktype="relative-path">remote procedure call</a>.
Sending this packet MUST tell the service provider the new set of media types
to detect for the indicated line (replacing any previous set). It MUST also set
the initial set of media types that SHOULD be monitored for on subsequent calls
(inbound or outbound) on this line.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Req_Func</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved1</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">hLine</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwMediaModes</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved2</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved3</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved4</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved5</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved6</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved7</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved8</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved9</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved10</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved11</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved12</p>
  </td>
 </tr>
</tbody></table><p><b>Req_Func (4 bytes): </b>An unsigned 32-bit
integer. The identifier of the function that will be invoked on the remote
server. This value MUST be set to 76.</p><dl>
<dd>
<p><b>Return Values</b></p>
</dd>
<dd>
<p>On completion of <a href="c28c36d0-579b-4e20-a100-f4e71012d5f8" data-linktype="relative-path">ClientRequest</a>, this field
MUST contain the result of the encapsulated telephony request. A value of 0
indicates success, and a <a href="e0e8af90-24f1-4dbc-8d4e-01b8e4e7cb53" data-linktype="relative-path">LINEERR_Constants</a>
value indicates failure. The remote server MUST complete this call
synchronously.</p>
</dd>
<dd>
<p>Returns zero if the function succeeds, or an error
number if an error occurs. Common return values are as follows:</p>
</dd>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Name</p>
   </th>
   <th>
   <p>Value</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>LINEERR_INVALLINEHANDLE</p>
  </td>
  <td>
  <p>0x8000002B</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONFAILED</p>
  </td>
  <td>
  <p>0x80000048</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_INVALMEDIAMODE</p>
  </td>
  <td>
  <p>0x8000002F</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_RESOURCEUNAVAIL</p>
  </td>
  <td>
  <p>0x8000004B</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_NOMEM</p>
  </td>
  <td>
  <p>0x80000044</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_NODRIVER</p>
  </td>
  <td>
  <p>0x80000043</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONUNAVAIL</p>
  </td>
  <td>
  <p>0x80000049</p>
  </td>
 </tr></tbody></table>
</dd></dl><p><b>Reserved1 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>hLine (4 bytes): </b>An <a href="9a80ee5c-cf55-4a86-bd67-173059d6ff3c" data-linktype="relative-path">HLINE</a>. The handle to the
line to have media monitoring set. This field MUST have been obtained by
sending the <a href="2759c744-e040-4c5d-b4b5-215d391f0490" data-linktype="relative-path">Open</a>
packet.</p><p><b>dwMediaModes (4 bytes): </b>An unsigned 32-bit
integer. The media types of interest to TAPI. This parameter MUST use one of
the <a href="e3b2104f-131d-4ead-9ded-45654ebfeac0" data-linktype="relative-path">LINEMEDIAMODE_Constants</a>.</p><p><b>Reserved2 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved3 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved4 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved5 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved6 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved7 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved8 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved9 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved10 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved11 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved12 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p></div>