<div class="content"><p>The <b>ROUTER_CONNECTION_STATE</b> type enumerates the
possible states of an interface on the RRAS server.</p><dl>
<dd>
<div><pre> typedef enum 
 {
   ROUTER_IF_STATE_UNREACHABLE,
   ROUTER_IF_STATE_DISCONNECTED,
   ROUTER_IF_STATE_CONNECTING,
   ROUTER_IF_STATE_CONNECTED
 } ROUTER_CONNECTION_STATE;
</pre></div>
</dd></dl><p><b>ROUTER_IF_STATE_UNREACHABLE: </b>The interface is
unreachable.</p><p><b>ROUTER_IF_STATE_DISCONNECTED: </b>The interface is
reachable but disconnected.</p><p><b>ROUTER_IF_STATE_CONNECTING: </b>The interface is
in the process of connecting.</p><p><b>ROUTER_IF_STATE_CONNECTED: </b>The interface is
connected.</p></div>