<div class="content"><p> </p><p>The fax client calls the <b>FaxObs_SetGlobalRoutingInfo
(Opnum 21)</b> method to set global routing properties, such as the routing
method priority.</p><p>In response, the server MUST validate that the client&#39;s fax
user account has access to set the global routing information. On success, the
server MUST modify its global fax routing method data, such as the routing
priority.</p><dl>
<dd>
<div><pre> error_status_t FaxObs_SetGlobalRoutingInfo(
   [in] handle_t hBinding,
   [in] const FAX_GLOBAL_ROUTING_INFOW* RoutingInfo
 );
</pre></div>
</dd></dl><p><b>hBinding: </b>The RPC binding handle for this
call. The client SHOULD reuse the RPC binding handle used as an input <i>hBinding</i>
argument for the <b>FaxObs_ConnectionRefCount</b> (section <span><a href="9430f7e2-d21d-4a38-a859-367b74f68a1a" data-linktype="relative-path">3.1.4.2.2</a></span>)
method call used to connect to the fax server.</p><p><b>RoutingInfo: </b>A pointer to a buffer that
contains a <b>FAX_GLOBAL_ROUTING_INFOW</b> (section <span><a href="4e1f24a1-5809-4fe2-93c8-6b12a35a5d6b" data-linktype="relative-path">2.2.32</a></span>)
structure.</p><p><b>Return Values: </b>This method MUST return
0x00000000 (ERROR_SUCCESS) for success; otherwise, it MUST return one of the
following error codes, one of the fax-specific errors that are defined in
section <span><a href="cbe6c4fb-4dda-4f6c-9701-0d490ba0d105" data-linktype="relative-path">2.2.52</a></span>, or one of
the other standard errors defined in <span><a href="../ms-erref/1bc92ddf-b79e-413c-bbaa-99a5281a6c90" data-linktype="relative-path">[MS-ERREF]</a></span>
section <span><a href="../ms-erref/18d8fbe8-a967-4f1c-ae50-99ca8e491d2d" data-linktype="relative-path">2.2</a></span>.</p><dl>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Return value/code</p>
   </th>
   <th>
   <p>Description</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>ERROR_ACCESS_DENIED</p>
  <p>0x00000005</p>
  </td>
  <td>
  <p>Access is denied. The client&#39;s fax user account does
  not have the FAX_CONFIG_SET access rights. </p>
  </td>
 </tr><tr>
  <td>
  <p>ERROR_INVALID_DATA</p>
  <p>0x0000000D</p>
  </td>
  <td>
  <p>The fax server cannot find the routing method
  specified by the <b>Guid</b> structure field of the <i>RoutingInfo</i>
  parameter.</p>
  </td>
 </tr><tr>
  <td>
  <p>ERROR_INVALID_PARAMETER</p>
  <p>0x00000057</p>
  </td>
  <td>
  <p>The parameter is incorrect. This error code is
  returned if any of the following conditions are met:</p>
  <p><span>§<span>  
  </span></span>The <i>RoutingInfo</i> is set to a NULL pointer value.</p>
  <p><span>§<span>  
  </span></span>The <b>SizeOfStruct</b> structure field of the <i>RoutingInfo</i>
  is not set to the correct size in bytes for the <b>FAX_GLOBAL_ROUTING_INFO</b>.</p>
  </td>
 </tr></tbody></table>
</dd></dl><p><b>Exceptions Thrown:</b> No exceptions are thrown
except those that are thrown by the underlying <span><a href="46aba9c4-ebb1-4b10-86ac-4bb3025657b9#gt_8a7f6700-8311-45bc-af10-82e10accd331" data-linktype="relative-path">RPC</a></span> protocol, <span><a href="../ms-rpce/290c38b1-92fe-4229-91e6-4fc376610c15" data-linktype="relative-path">[MS-RPCE]</a></span>.</p></div>