<div class="content"><p>The <b>IP_AUTO_DHCP_INTERFACE_INFO</b> structure holds
per-interface configuration for the DHCP allocator. This structure is used in
the following methods:</p><ul><li><p><span><span> 
</span></span><a href="927c5bf1-ac91-4325-b945-0d96a58f609b" data-linktype="relative-path"><b>RRouterInterfaceTransportAdd (section 3.1.4.18)</b></a><span>  </span></p>
</li><li><p><span><span> 
</span></span><a href="ec9ba293-45e9-4f12-b9af-7e77ec96c90e" data-linktype="relative-path"><b>RRouterInterfaceTransportGetInfo (section 3.1.4.19)</b></a><span>  </span></p>
</li><li><p><span><span> 
</span></span><a href="209ba5e7-876e-4406-a05c-65b7e5fb2380" data-linktype="relative-path"><b>RRouterInterfaceTransportSetInfo (section 3.1.4.20)</b></a><span>  </span></p>
</li></ul><p>The configuration only allows the DHCP allocator to be
disabled on the given interface. Since the allocator runs in
promiscuous-interface mode, it is enabled by default on all interfaces. Thus,
the only interfaces that require any configuration are those on which the
allocator is to be disabled.</p><dl>
<dd>
<div><pre> typedef struct _IP_AUTO_DHCP_INTERFACE_INFO {
   ULONG Flags;
 } IP_AUTO_DHCP_INTERFACE_INFO,
  *PIP_AUTO_DHCP_INTERFACE_INFO;
</pre></div>
</dd></dl><p><b>Flags: </b>Specifies whether or not the DHCP
allocator is enabled.</p><dl>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Value</p>
   </th>
   <th>
   <p>Meaning</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>0x00000000</p>
  </td>
  <td>
  <p>The DHCP allocator is enabled.</p>
  </td>
 </tr><tr>
  <td>
  <p>IPNATHLP_INTERFACE_FLAG_DISABLED</p>
  <p>0x00000001</p>
  </td>
  <td>
  <p>The DHCP allocator is disabled.</p>
  </td>
 </tr></tbody></table>
</dd></dl><p> </p></div>