<div class="content"><p>The NtmsMountOptions enumeration defines options for <a href="8d988f06-72be-47cf-9e09-9060aa8ed897#gt_cc98b88f-7fd4-40f6-b315-212dc4d8378b" data-linktype="relative-path">mount</a> operations.</p><dl>
<dd>
<div><pre> enum NtmsMountOptions
 {
   NTMS_MOUNT_READ = 0x0001,
   NTMS_MOUNT_WRITE = 0x0002,
   NTMS_MOUNT_ERROR_NOT_AVAILABLE = 0x0004,
   NTMS_MOUNT_ERROR_OFFLINE = 0x0008,
   NTMS_MOUNT_SPECIFIC_DRIVE = 0x0010,
   NTMS_MOUNT_NOWAIT = 0x0020
 };
</pre></div>
</dd></dl><p><b>NTMS_MOUNT_READ:  </b>Mount the media with read
access enabled.</p><p><b>NTMS_MOUNT_WRITE:  </b>Mount the media with write
access enabled. Media that are marked as completed MUST NOT be mounted with
write access enabled.</p><p><b>NTMS_MOUNT_ERROR_NOT_AVAILABLE:  </b>Return an
error if the media or a <a href="8d988f06-72be-47cf-9e09-9060aa8ed897#gt_1112c690-ee01-4c9b-aa55-9569fd82178b" data-linktype="relative-path">drive</a>
is not available.</p><p><b>NTMS_MOUNT_ERROR_OFFLINE:  </b>Return an error if
the media specified is not currently in an online library.</p><p><b>NTMS_MOUNT_SPECIFIC_DRIVE:  </b>Mount the media
into the drives.</p><p><b>NTMS_MOUNT_NOWAIT:  </b>Specify that the server
MUST NOT wait for the mount request to complete.</p></div>