<div class="content"><p>The AASYNDATARESP structure contains the RDGUDP channel
properties sent by the RDG <a href="76796f19-9e6f-48b9-8b8f-4ef9f197056b#gt_434b0234-e970-4e8c-bdfa-e16a30d96703" data-linktype="relative-path">server</a>
to the RDG <a href="76796f19-9e6f-48b9-8b8f-4ef9f197056b#gt_60e0e1fa-66fe-41e1-b5e3-ceab97e53506" data-linktype="relative-path">client</a> during
the <a href="0fcd8c37-7540-426a-a385-8e6be22611fc" data-linktype="relative-path">Connection Setup
Phase (section 1.3.1.1.1)</a>.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="16">
  <p>uUpStreamMtu</p>
  </td>
  <td colspan="16">
  <p>uDownStreamMtu</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>snRecvISN</p>
  </td>
 </tr>
</tbody></table><p><b>uUpStreamMtu (2 bytes): </b>An unsigned short
representing the resultant path for the <a href="76796f19-9e6f-48b9-8b8f-4ef9f197056b#gt_03aae42f-32fd-47ab-b413-d5ec92d29d45" data-linktype="relative-path">MTU</a> between the RDG client,
the RDG server and the <a href="76796f19-9e6f-48b9-8b8f-4ef9f197056b#gt_3657ab68-5a60-4cee-8082-dfc2e67435e9" data-linktype="relative-path">target
server</a>. The path is detected by the RDG server after establishing a
connection with the target server.</p><p><b>uDownStreamMtu (2 bytes): </b>An unsigned short
representing the resultant path for the MTU between the target server, the RDG
server and the RDG client. The path is detected by the RDG server after
establishing a connection with the target server.</p><p><b>snRecvISN (4 bytes): </b>An integer representing
the initial sequence number used by the forward error correction (FEC) receive
window between the target server and the RDG client. The integer value is sent
by the target server to the RDG server during the Connection Setup Phase.</p></div>