<div class="content"><p>The DevSpecificFeature packet is transmitted from a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_60e0e1fa-66fe-41e1-b5e3-ceab97e53506" data-linktype="relative-path">client</a> to a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_434b0234-e970-4e8c-bdfa-e16a30d96703" data-linktype="relative-path">server</a> in a <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_8a7f6700-8311-45bc-af10-82e10accd331" data-linktype="relative-path">remote procedure call</a>. The
function is used as an extension mechanism to enable service providers to
provide access to features that are not described in other operations. The
meanings of these extensions are device-specific, and taking advantage of these
extensions requires TAPI or its client application to be fully aware of them.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Req_Func</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved1</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwRequestID</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">lpContext</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">hLine</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwFeature</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">lpParamsContext</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">lpParams</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwSize</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved2</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved3</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved4</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved5</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved6</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved7</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">VarData
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">...</p>
  </td>
 </tr>
</tbody></table><p><b>Req_Func (4 bytes): </b>The identifier of the
function that will be invoked on the remote server. This value MUST be set to
14.</p><dl>
<dd>
<p><b>Return Values</b></p>
</dd>
<dd>
<p>On completion of <a href="c28c36d0-579b-4e20-a100-f4e71012d5f8" data-linktype="relative-path">ClientRequest</a>, this field
contains the result of the encapsulated telephony request. A nonzero request ID
value indicates that the request is in progress and will complete
asynchronously, and a <a href="e0e8af90-24f1-4dbc-8d4e-01b8e4e7cb53" data-linktype="relative-path">LINEERR_Constants</a>
value indicates synchronous failure.</p>
</dd>
<dd>
<p>Returns a positive request identifier if the
function will be completed asynchronously or a negative error number if an
error occurs. The dwParam2 parameter of the corresponding <a href="8f5bc349-fd55-46f2-b0bc-dc9f757317a9" data-linktype="relative-path">LINE_REPLY</a> packet is zero
if the function succeeds, or it is a negative error number if an error occurs.
If the client specified a nonzero value in the dwRequestID field of the packet,
the same MUST be used as the value for the returned positive request
identifier. Common return values are as follows:</p>
</dd>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Name</p>
   </th>
   <th>
   <p>Value</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>LINEERR_INVALFEATURE</p>
  </td>
  <td>
  <p>0x80000055</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONUNAVAIL</p>
  </td>
  <td>
  <p>0x80000049</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_INVALLINEHANDLE</p>
  </td>
  <td>
  <p>0x8000002B</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONFAILED</p>
  </td>
  <td>
  <p>0x80000048</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_NOMEM</p>
  </td>
  <td>
  <p>0x80000044</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_RESOURCEUNAVAIL</p>
  </td>
  <td>
  <p>0x8000004B</p>
  </td>
 </tr></tbody></table>
</dd></dl><p><b>Reserved1 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>dwRequestID (4 bytes): </b>An unsigned 32-bit
integer. The identifier of the asynchronous request.</p><p><b>lpContext (4 bytes): </b>An unsigned 32-bit
integer. The opaque, client-specified value that is used by the client upon
request completion; MUST be returned by the server in the request completion
packet.</p><p><b>hLine (4 bytes): </b>An <a href="9a80ee5c-cf55-4a86-bd67-173059d6ff3c" data-linktype="relative-path">HLINE</a>. The handle to the
line device. This field MUST have been obtained by sending the <a href="2759c744-e040-4c5d-b4b5-215d391f0490" data-linktype="relative-path">Open</a> packet.</p><p><b>dwFeature (4 bytes): </b>An unsigned 32-bit
integer. The feature to invoke on the line device. This parameter MUST use <a href="288e9937-76f8-4bc6-8a6d-9e4abe6d56b0" data-linktype="relative-path">PHONEBUTTONFUNCTION_Constants</a>.</p><p><b>lpParamsContext (4 bytes): </b>An unsigned 32-bit
integer. The opaque, client-specified value that is used by the client upon
request completion; MUST be returned by the server in the request completion
packet.</p><p><b>lpParams (4 bytes): </b>An unsigned 32-bit
integer. The offset, in bytes, in the VarData field of a feature-dependent
parameter block. The format of this parameter block is device-specific and its
contents are passed by TAPI, to or from the TSP.</p><p><b>dwSize (4 bytes): </b>An unsigned 32-bit integer.
The size, in bytes, of the parameter block that is indicated in the lpParams
field.</p><p><b>Reserved2 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved3 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved4 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved5 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved6 (4 bytes): </b>An unsigned 32-bit integer.
This field is used for padding and MUST be ignored on receipt. It can be any
value.</p><p><b>Reserved7 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>VarData (variable): </b>Contains a
feature-dependent parameter block that is indicated in the lpParams field. The
format of this parameter block is device-specific and its contents are passed
by TAPI, to or from the TSP.</p><dl>
<dd>
<p>The contents of this field MUST be DWORD-aligned, as
specified in <a href="../ms-dtyp/cca27429-5689-4a16-b2b4-9325d93e4ba2" data-linktype="relative-path">[MS-DTYP]</a>
section <a href="../ms-dtyp/262627d8-3418-4627-9218-4ffe110850b2" data-linktype="relative-path">2.2.9</a>.</p>
</dd></dl></div>