<div class="content"><p>The <b>MIB_UDPTABLE</b> structure contains a table of
address information for sending and receiving UDP datagrams on the local
computer.</p><dl>
<dd>
<div><pre> typedef struct _MIB_UDPTABLE {
   DWORD dwNumEntries;
   MIB_UDPROW table[1];
   BYTE reserved[8];
 } MIB_UDPTABLE,
  *PMIB_UDPTABLE;
</pre></div>
</dd></dl><p><b>dwNumEntries: </b>The number of entries in the
table.</p><p><b>table: </b>Pointer to an array of
MIB_UDPROW (section <a href="451bb64e-496e-4887-89c5-171b6d10f6ee" data-linktype="relative-path">2.2.1.2.58</a>)
structures.</p><p><b>reserved: </b>An array of 8 bytes that SHOULD be
set to 0 and ignored on receipt.</p></div>