<div class="content"><p>The GetAddressStatus packet is transmitted from a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_60e0e1fa-66fe-41e1-b5e3-ceab97e53506" data-linktype="relative-path">client</a> to a TAPI <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_434b0234-e970-4e8c-bdfa-e16a30d96703" data-linktype="relative-path">server</a> in a <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_8a7f6700-8311-45bc-af10-82e10accd331" data-linktype="relative-path">remote procedure call</a>.
Sending this packet queries the specified address for its current status.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Req_Func</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved1</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">hLine</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwAddressID</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">lpAddressStatus</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved2</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved3</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved4</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved5</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved6</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved7</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved8</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved9</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved10</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved11</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">VarData
  (64 bytes, optional)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">...</p>
  </td>
 </tr>
</tbody></table><p><b>Req_Func (4 bytes): </b>An unsigned 32-bit
integer. The identifier of the function that will be invoked on the remote
server. This value MUST be set to 23.</p><dl>
<dd>
<p><b>Return Values</b></p>
</dd>
<dd>
<p>On completion of <a href="c28c36d0-579b-4e20-a100-f4e71012d5f8" data-linktype="relative-path">ClientRequest</a>, this field
will contain the result of the encapsulated telephony request. A value of 0
indicates success and a <a href="e0e8af90-24f1-4dbc-8d4e-01b8e4e7cb53" data-linktype="relative-path">LINEERR_Constants</a>
value indicates failure. The remote server MUST complete this call
synchronously.</p>
</dd>
<dd>
<p>MUST return zero if the function succeeds or an
error number if an error occurs. Common return values are as follows:</p>
</dd>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Name</p>
   </th>
   <th>
   <p>Value</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>LINEERR_INVALLINEHANDLE</p>
  </td>
  <td>
  <p>0x8000002B</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONUNAVAIL</p>
  </td>
  <td>
  <p>0x80000049</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_INVALADDRESSID</p>
  </td>
  <td>
  <p>0x80000011</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_OPERATIONFAILED</p>
  </td>
  <td>
  <p>0x80000048</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_NOMEM</p>
  </td>
  <td>
  <p>0x80000044</p>
  </td>
 </tr><tr>
  <td>
  <p>LINEERR_RESOURCEUNAVAIL</p>
  </td>
  <td>
  <p>0x8000004B</p>
  </td>
 </tr></tbody></table>
</dd></dl><p><b>Reserved1 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>hLine (4 bytes): </b>An <a href="9a80ee5c-cf55-4a86-bd67-173059d6ff3c" data-linktype="relative-path">HLINE</a>. The handle to the
opened line device that contains the address to query. This field MUST have
been obtained by sending the <a href="2759c744-e040-4c5d-b4b5-215d391f0490" data-linktype="relative-path">Open</a>
packet.</p><p><b>dwAddressID (4 bytes): </b>An unsigned 32-bit
integer. An address on the particular open line device. This is the address to
be queried. An address identifier is permanently associated with an address;
the identifier remains constant across operating system upgrades. A valid value
of dwAddressID is in the range 0 to dwNumAddresses –1. The client obtains
dwNumAddresses from the <a href="f236ea7a-c8a2-4681-b87c-9f0e07a01dc6" data-linktype="relative-path">LINEDEVCAPS</a>
obtained by sending a <a href="ee317c21-100e-48a3-bcce-e9991efff889" data-linktype="relative-path">GetDevCaps</a>
packet to the remote server.  This parameter is not validated by TAPI when this
function is called.</p><p><b>lpAddressStatus (4 bytes): </b>An unsigned 32-bit
integer. The size of a <a href="f268e780-6bbf-4640-bbfe-0907045e032a" data-linktype="relative-path">LINEADDRESSSTATUS</a>
packet that, upon successful completion of the request, contains the current
status of an address. Upon successful completion, this field contains the
offset, in bytes, of the packet in the VarData field.</p><p><b>Reserved2 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved3 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved4 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved5 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved6 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved7 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved8 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved9 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved10 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>Reserved11 (4 bytes): </b>An unsigned 32-bit
integer. This field is used for padding and MUST be ignored on receipt. It can
be any value.</p><p><b>VarData (64 bytes): </b>This field is only present
on successful completion of the request. Contains a LINEADDRESSSTATUS packet.</p><dl>
<dd>
<p>The contents of this field MUST be DWORD-aligned, as
specified in <a href="../ms-dtyp/cca27429-5689-4a16-b2b4-9325d93e4ba2" data-linktype="relative-path">[MS-DTYP]</a>
section <a href="../ms-dtyp/262627d8-3418-4627-9218-4ffe110850b2" data-linktype="relative-path">2.2.9</a>.</p>
</dd></dl></div>