<div class="content"><p>The <b>DIM_MIB_ENTRY_CONTAINER</b> structure contains the
size and the data for the management information base (MIB) entries that are
either set or retrieved from the MIB variables. This structure is used in the
following methods:</p><ul><li><p><span><span> 
</span></span><a href="4a8dc1a9-4b2a-4eba-bd0e-df9e8dc97908" data-linktype="relative-path"><b>RMIBEntryCreate (section 3.1.4.27)</b></a></p>
</li><li><p><span><span> 
</span></span><a href="a8ed0e17-9395-4aef-9f4e-9b3e93cf3f4c" data-linktype="relative-path"><b>RMIBEntryDelete (section 3.1.4.28)</b></a></p>
</li><li><p><span><span> 
</span></span><a href="61ae7aea-8604-4bf3-8ae5-88542152cf8e" data-linktype="relative-path"><b>RMIBEntrySet (section 3.1.4.29)</b></a></p>
</li><li><p><span><span> 
</span></span><a href="ebc5c709-36d8-4520-a0ac-6f36d2d6c0b2" data-linktype="relative-path"><b>RMIBEntryGet (section 3.1.4.30)</b></a></p>
</li><li><p><span><span> 
</span></span><a href="9102e585-2f62-4408-bfb6-02a6460cc883" data-linktype="relative-path"><b>RMIBEntryGetFirst (section 3.1.4.31)</b></a></p>
</li><li><p><span><span> 
</span></span><a href="50f78033-d248-4272-b4b9-a2519a0f304d" data-linktype="relative-path"><b>RMIBEntryGetNext (section 3.1.4.32)</b></a></p>
<div><pre> typedef struct _DIM_MIB_ENTRY_CONTAINER 
 {
   DWORD dwMibInEntrySize;
   [size_is(dwMibInEntrySize)] LPBYTE pMibInEntry;
   DWORD dwMibOutEntrySize;
   [size_is(dwMibOutEntrySize)] LPBYTE pMibOutEntry;
 } DIM_MIB_ENTRY_CONTAINER,
  *PDIM_MIB_ENTRY_CONTAINER;
</pre></div>
</li></ul><p><b>dwMibInEntrySize: </b>This field gives the size of
the MIB entry data being input. It represents the size of the data contained in
<b>pMibInEntry</b>.</p><p><b>pMibInEntry: </b>A pointer to a protocol-specific
structure that contains input data.</p><p><b>dwMibOutEntrySize: </b>This field gives the size
of the MIB entry data being output. It represents the size of the data
contained in <b>pMibOutEntry</b>.</p><p><b>pMibOutEntry: </b>This member points to the
protocol-specific structure that points to the MIB.</p><dl>
<dd>
<p>The contents of pMibInEntry and pMibOutEntry are
based on the transport and the routing protocol for which the MIB information
is requested.</p>
</dd>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Transport</p>
   </th>
   <th>
   <p>Routing Protocol</p>
   </th>
   <th>
   <p>pMibInEntry</p>
   </th>
   <th>
   <p>pMibOutEntry</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>PID_IP</p>
  <p>0x00000021</p>
  </td>
  <td>
  <p>IPRTRMGR_PID</p>
  <p>0x00002710</p>
  </td>
  <td>
  <p>MIB_OPAQUE_QUERY (section <a href="3ca0723e-36ea-448a-a97e-1906dd3d07a6" data-linktype="relative-path">2.2.1.2.53</a>)</p>
  </td>
  <td>
  <p>MIB_OPAQUE_QUERY (section 2.2.1.2.53)</p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IP</p>
  <p>0x00000021</p>
  </td>
  <td>
  <p>MS_IP_BOOTP</p>
  <p>0x0000270F</p>
  </td>
  <td>
  <p><a href="1ae16359-49ce-4b60-bb00-33413aa77ec5" data-linktype="relative-path">IPBOOT_MIB_GET_INPUT_DATA (section 2.2.1.2.151)</a></p>
  </td>
  <td>
  <p><a href="46db75a0-7e95-490e-aac5-c8c96df8c57c" data-linktype="relative-path">IPBOOTP_MIB_GET_OUTPUT_DATA (section 2.2.1.2.152)</a></p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IP</p>
  <p>0x00000021</p>
  </td>
  <td>
  <p>MS_IP_NAT</p>
  <p>0x81372715</p>
  </td>
  <td>
  <p><a href="02a17b1a-22a6-4295-bc7d-f3b781c01332" data-linktype="relative-path">IP_NAT_MIB_QUERY (section 2.2.1.2.182)</a></p>
  </td>
  <td>
  <p>IP_NAT_MIB_QUERY (section 2.2.1.2.182)</p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IP</p>
  <p>0x00000021</p>
  </td>
  <td>
  <p>MS_IP_DNS_PROXY</p>
  <p>0x81372713</p>
  </td>
  <td>
  <p>IP_DNS_PROXY_MIB_QUERY (section <a href="c22770ac-2b26-4bdb-bb1c-2b742d4d4a9d" data-linktype="relative-path">2.2.1.2.186)</a></p>
  </td>
  <td>
  <p>IP_DNS_PROXY_MIB_QUERY (section 2.2.1.2.186)</p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IP</p>
  <p>0x00000021</p>
  </td>
  <td>
  <p>MS_IP_DHCP_ALLOCATOR</p>
  <p>0x81372714</p>
  </td>
  <td>
  <p>IP_AUTO_DHCP_MIB_QUERY (section <a href="a85fd7a5-b937-4daa-a703-a0c1fcb0069a" data-linktype="relative-path">2.2.1.2.188)</a></p>
  </td>
  <td>
  <p>IP_AUTO_DHCP_MIB_QUERY (section 2.2.1.2.188)</p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IP</p>
  <p>0x00000021</p>
  </td>
  <td>
  <p>MS_IP_OSPF</p>
  <p>0x0000000D</p>
  </td>
  <td>
  <p>MIB_DA_MSG (section <a href="3ed7b98d-09e8-4113-99b0-4ed4b6cf6c01" data-linktype="relative-path">2.2.1.2.190)</a></p>
  </td>
  <td>
  <p>MIB_DA_MSG (section 2.2.1.2.190)</p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IP</p>
  <p>0x00000021</p>
  </td>
  <td>
  <p>MS_IP_RIP</p>
  <p>0x00000008</p>
  </td>
  <td>
  <p><a href="45250002-d774-4bc2-ab2e-6992341b5f45" data-linktype="relative-path">IPRIP_MIB_GET_INPUT_DATA (section 2.2.1.2.161)</a></p>
  </td>
  <td>
  <p><a href="4fc16996-6de7-4f99-8cea-40e1f42931e1" data-linktype="relative-path">IPRIP_MIB_GET_OUTPUT_DATA (section 2.2.1.2.162)</a></p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IP</p>
  <p>0x00000021</p>
  </td>
  <td>
  <p>MS_IP_IGMP</p>
  <p>0x4137000A</p>
  </td>
  <td>
  <p><a href="7a931cdc-e37b-4bf5-ac39-34cdded2dd49" data-linktype="relative-path">IGMP_MIB_GET_INPUT_DATA (section 2.2.1.2.171)</a></p>
  </td>
  <td>
  <p><a href="78cfd91f-a654-4a17-8493-cbd25ae799a8" data-linktype="relative-path">IGMP_MIB_GET_OUTPUT_DATA (section 2.2.1.2.172)</a></p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IPV6</p>
  <p>0x00000057</p>
  </td>
  <td>
  <p>MS_IPV6_DHCP</p>
  <p>0x000003E7</p>
  </td>
  <td>
  <p><a href="c16ecd43-fa27-4146-a55b-5721f6500f2f" data-linktype="relative-path">DHCPV6R_MIB_GET_INPUT_DATA (section 2.2.1.2.160)</a></p>
  </td>
  <td>
  <p><a href="f841e214-2cfe-4265-9867-bd1cb685936b" data-linktype="relative-path">DHCPV6R_MIB_GET_OUTPUT_DATA (section 2.2.1.2.156)</a></p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IPV6</p>
  <p>0x00000057</p>
  </td>
  <td>
  <p>IPRTRMGR_PID</p>
  <p>0x00002710</p>
  </td>
  <td>
  <p>MIB_OPAQUE_QUERY (section 2.2.1.2.53)</p>
  </td>
  <td>
  <p>MIB_OPAQUE_QUERY (section 2.2.1.2.53)</p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IPX</p>
  <p>0x0000002B</p>
  </td>
  <td>
  <p>IPX_PROTOCOL_BASE</p>
  <p>0x0001FFFF</p>
  </td>
  <td>
  <p><a href="25b333ba-d914-4569-9abe-c2be448d09a0" data-linktype="relative-path">IPX_MIB_GET_INPUT_DATA (section 2.2.1.2.105)</a></p>
  </td>
  <td>
  <p>IPX_MIB_GET_INPUT_DATA (section 2.2.1.2.105)</p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IPX</p>
  <p>0x0000002B</p>
  </td>
  <td>
  <p>IPX_PROTOCOL_RIP</p>
  <p>0x00020000</p>
  </td>
  <td>
  <p><a href="d7f3b4c1-68d3-49ca-b514-7300927d905a" data-linktype="relative-path">RIP_MIB_GET_INPUT_DATA (section 2.2.1.2.125)</a></p>
  </td>
  <td>
  <p>RIP_MIB_GET_INPUT_DATA (section 2.2.1.2.125)</p>
  </td>
 </tr><tr>
  <td>
  <p>PID_IPX</p>
  <p>0x0000002B</p>
  </td>
  <td>
  <p>IPX_PROTOCOL_SAP</p>
  <p>0x00020000</p>
  </td>
  <td>
  <p><a href="341d9227-3a24-428a-ac46-dd076dcacac6" data-linktype="relative-path">SAP_MIB_GET_INPUT_DATA (section 2.2.1.2.118)</a></p>
  </td>
  <td>
  <p>SAP_MIB_GET_INPUT_DATA (section 2.2.1.2.118)</p>
  </td>
 </tr></tbody></table>
</dd></dl><p> </p></div>