<div class="content"><p>RpcGetForm retrieves information about a specified form.</p><dl>
<dd>
<div><pre> DWORD RpcGetForm(
   [in] PRINTER_HANDLE hPrinter,
   [in, string] wchar_t* pFormName,
   [in] DWORD Level,
   [in, out, unique, size_is(cbBuf), disable_consistency_check] 
     BYTE* pForm,
   [in] DWORD cbBuf,
   [out] DWORD* pcbNeeded
 );
</pre></div>
</dd></dl><p><b>hPrinter: </b>A handle to a printer object or
server object that was opened by <a href="bd0bb8d5-26fd-4705-81f5-614d32b9f38f" data-linktype="relative-path">RpcAddPrinter (section 3.1.4.2.3)</a>,
<a href="3af45717-308f-4b4f-8428-430d12856110" data-linktype="relative-path">RpcAddPrinterEx (section 3.1.4.2.15)</a>,
<a href="989357e2-446e-4872-bb38-1dce21e1313f" data-linktype="relative-path">RpcOpenPrinter (section 3.1.4.2.2)</a>,
or <a href="0e81ce18-72b1-46c3-8584-a205393b04ff" data-linktype="relative-path">RpcOpenPrinterEx (section 3.1.4.2.14)</a>.</p><p><b>pFormName: </b>A pointer to a string that
specifies the form name for which data is required. For rules governing form
names, see section <a href="cd213afb-1b67-4479-ac15-316ea0fb537e" data-linktype="relative-path">2.2.4.5</a>.</p><p><b>Level: </b>The form information level.</p><dl>
<dd>
<table><thead>
  <tr>
   <th>
   <p>Value</p>
   </th>
   <th>
   <p>Description</p>
   </th>
  </tr>
 </thead><tbody><tr>
  <td>
  <p>0x00000001</p>
  </td>
  <td>
  <p>Corresponds to <a href="95e918de-fbdb-4d0a-ad4c-d7005ab33305" data-linktype="relative-path">_FORM_INFO_1 (section 2.2.2.5.1)</a>.</p>
  </td>
 </tr><tr>
  <td>
  <p>0x00000002</p>
  </td>
  <td>
  <p>Corresponds to <a href="b15260d2-493c-49ac-9062-720162e1aee1" data-linktype="relative-path">_FORM_INFO_2 (section 2.2.2.5.2)</a>.</p>
  </td>
 </tr></tbody></table>
</dd></dl><p><b>pForm: </b>A pointer to the <a href="f29e9057-df29-40d4-9c51-c615c0da62a1" data-linktype="relative-path">BUFFER</a>, as specified in
INFO Structures Query Parameters (section 3.1.4.1.9).</p><p><b>BUFFER TYPE:</b> _FORM_INFO.</p><dl>
<dd>
<p>This parameter can be NULL if <i>cbBuf</i> equals
zero.</p>
</dd></dl><p><b>cbBuf: </b>Specified in INFO Structures Query Parameters.</p><p><b>pcbNeeded: </b>Specified in INFO Structures Query
Parameters.</p><p><b>Return Values: </b>This method MUST return zero
(ERROR_SUCCESS) to indicate successful completion or a nonzero Windows error
code to indicate failure <a href="../ms-erref/1bc92ddf-b79e-413c-bbaa-99a5281a6c90" data-linktype="relative-path">[MS-ERREF]</a>.</p><p>Upon receiving this message, the server MUST validate
parameters as follows:</p><ul><li><p><span><span> 
</span></span>Perform the validation steps that are specified in <a href="10bfa8c2-d456-4ad0-912d-e674766a36c8" data-linktype="relative-path">PRINTER_HANDLE Parameters (section 3.1.4.1.11)</a>.
This method SHOULD assume that the handle to the printer or server object can
be used without further access checks.</p>
</li><li><p><span><span> 
</span></span>Verify that the <i>pFormName</i> parameter points to a string
that identifies an existing form. If that verification fails, return
ERROR_INVALID_FORM_NAME [MS-ERREF].</p>
</li><li><p><span><span> 
</span></span>Perform the validation steps specified in INFO Structures Query
Parameters.</p>
</li></ul><p>If parameter validation fails, the server MUST fail the
operation immediately and return a nonzero error response to the client. Otherwise,
the server MUST process the message and compose a response to the client as
follows:</p><ul><li><p><span><span> 
</span></span>Using information about the form, perform the processing and
response steps specified in INFO Structures Query Parameters.</p>
</li><li><p><span><span> 
</span></span>Return the status of the operation.</p>
</li></ul></div>