<div class="content"><p>The GetPhoneInfo packet queries information that pertains to
the phone device.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Req_Func</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved1</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">hPhoneApp</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">lpDeviceInfoList</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved2</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved3</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved4</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved5</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved6</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved7</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved8</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved9</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved10</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved11</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved12</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">VarData
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">...</p>
  </td>
 </tr>
</tbody></table><p><b>Req_Func (4 bytes): </b>The identifier of the
function that will be invoked on the remote <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_434b0234-e970-4e8c-bdfa-e16a30d96703" data-linktype="relative-path">server</a>. This value MUST be
set to 133.</p><dl>
<dd>
<p>On completion of <a href="c28c36d0-579b-4e20-a100-f4e71012d5f8" data-linktype="relative-path">ClientRequest</a>, this field
MUST contain the result of the encapsulated telephony request. A value of zero
indicates success, and a <a href="e0e8af90-24f1-4dbc-8d4e-01b8e4e7cb53" data-linktype="relative-path">LINEERR_Constants</a>
value indicates failure. The remote server MUST complete this call
synchronously.</p>
</dd></dl><p><b>Reserved1 (4 bytes): </b>An unsigned 32-bit integer.
MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>hPhoneApp (4 bytes): </b>An <a href="55b72ff6-9236-401b-846a-e8a78dfada1b" data-linktype="relative-path">HPHONEAPP</a>. The handle to
the application registration with TAPI. This field MUST have been obtained by
sending the <a href="a600d262-0bb1-447b-8a0d-6f57d3a8ec18" data-linktype="relative-path">Initialize</a>
packet.</p><p><b>lpDeviceInfoList (4 bytes): </b>An unsigned 32-bit
integer. The size of a <a href="21f70f2e-86e7-4ce2-a82d-6c4b0c20cfa0" data-linktype="relative-path">DEVICEINFOLIST</a>
packet that, upon successful completion of the request, MUST contain a list of
device information entries.</p><dl>
<dd>
<p>Upon successful completion, this field MUST contain
the offset, in bytes, of the packet in the VarData field.</p>
</dd></dl><p><b>Reserved2 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Reserved3 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Reserved4 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Reserved5 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Reserved6 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Reserved7 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Reserved8 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Reserved9 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Reserved10 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Reserved11 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Reserved12 (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>VarData (variable): </b>MUST contain a
DEVICEINFOLIST packet. The contents of this field are <a href="../ms-dtyp/262627d8-3418-4627-9218-4ffe110850b2" data-linktype="relative-path">DWORD</a>-aligned.
</p></div>