<div class="content"><p>The LINE_CREATE packet is sent to inform the application of
the creation of a new line device.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">TotalSize</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">InitContext</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">fnPostProcessProcHandle</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">hDevice</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Msg</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">OpenContext</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Param1</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Param2</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Param3</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Param4</p>
  </td>
 </tr>
</tbody></table><p><b>TotalSize (4 bytes): </b>An unsigned 32-bit
integer. The total size of the asynchronous event packet.</p><p><b>InitContext (4 bytes): </b>An unsigned 32-bit
integer. The opaque, client-specified session value that MUST be equal to the
InitContext value that is specified in the original scoping of the line <a href="9d8eb7cd-3245-4e44-97e0-42f7b89c9424" data-linktype="relative-path">Initialize</a> request.</p><p><b>fnPostProcessProcHandle (4 bytes): </b>An unsigned
32-bit integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>hDevice (4 bytes): </b>An unsigned 32-bit integer.
MUST be set to zero when sent and MUST be ignored on receipt.</p><p><b>Msg (4 bytes): </b>An unsigned 32-bit integer. The
packet type; MUST be set to 0x00000013 (LINE_CREATE).</p><p><b>OpenContext (4 bytes): </b>An unsigned 32-bit
integer. MUST be set to zero when sent and MUST be ignored on receipt. </p><p><b>Param1 (4 bytes): </b>An unsigned 32-bit integer.
The device identifier of the newly created device.</p><p><b>Param2 (4 bytes): </b>An unsigned 32-bit integer.
This MUST be ignored on receipt and can be any value.  </p><p><b>Param3 (4 bytes): </b>An unsigned 32-bit integer.
This MUST be ignored on receipt and can be any value.  </p><p><b>Param4 (4 bytes): </b>An unsigned 32-bit integer.
This MUST be ignored on receipt and can be any value.  </p></div>