<div class="content"><p> </p><p>The <b>FAX_SERVER_ACTIVITY</b> structure defines information
about the server&#39;s <span><a href="46aba9c4-ebb1-4b10-86ac-4bb3025657b9#gt_0c5e7185-40c3-4e58-a8ac-7626ed078235" data-linktype="relative-path">fax queue</a></span> activity
and the events reported by the fax server. This structure is used as an argument
for <b>FAX_GetServerActivity</b> (section <span><a href="ac6ac87f-f612-4d90-8d2a-64528c07d153" data-linktype="relative-path">3.1.4.1.61</a></span>).</p><dl>
<dd>
<div><pre> typedef struct {
   DWORD dwSizeOfStruct;
   DWORD dwIncomingMessages;
   DWORD dwRoutingMessages;
   DWORD dwOutgoingMessages;
   DWORD dwDelegatedOutgoingMessages;
   DWORD dwQueuedMessages;
   DWORD dwErrorEvents;
   DWORD dwWarningEvents;
   DWORD dwInformationEvents;
 } FAX_SERVER_ACTIVITY,
  *PFAX_SERVER_ACTIVITY;
</pre></div>
</dd></dl><p><b>dwSizeOfStruct:</b> A <b>DWORD</b> (<span><a href="../ms-dtyp/cca27429-5689-4a16-b2b4-9325d93e4ba2" data-linktype="relative-path">[MS-DTYP]</a></span>
section <span><a href="../ms-dtyp/262627d8-3418-4627-9218-4ffe110850b2" data-linktype="relative-path">2.2.9</a></span>)
value that holds the total size of the structure, in bytes. This value MUST be
36 bytes.</p><p><b>dwIncomingMessages:</b> A <b>DWORD</b> that
indicates the number of messages currently being received by the fax server.
This variable MAY also be set to the count of the number of incoming messages
that were successfully received and are currently being routed using an inbound
<span><a href="46aba9c4-ebb1-4b10-86ac-4bb3025657b9#gt_efaa1290-6d4b-4f44-9e84-35a867069d45" data-linktype="relative-path">routing</a></span>
method. If the routing fails, the incoming job SHOULD be marked for a routing
retry and the <b>dwRoutingMessages</b> member used to count this job when the
routing restarts. If this value is nonzero, stopping the server MAY result in
the loss of incoming messages.</p><p><b>dwRoutingMessages:</b> A <b>DWORD</b> that
indicates the number of incoming messages being rerouted after a routing
failure.</p><p><b>dwOutgoingMessages:</b> A <b>DWORD</b> that
indicates the number of messages currently being sent by the fax server. If
this value is nonzero, stopping the server MAY result in the loss of outgoing
messages.</p><p><b>dwDelegatedOutgoingMessages:</b> A <b>DWORD</b>
that indicates the number of messages currently being sent by a <span><a href="46aba9c4-ebb1-4b10-86ac-4bb3025657b9#gt_2ba66d72-d766-440f-b5ea-0333759b147c" data-linktype="relative-path">Fax
Service Provider</a></span> on behalf of the fax server. The fax server is not
currently sending these messages.</p><p><b>dwQueuedMessages:</b> A <b>DWORD</b> that
indicates the number of outgoing messages waiting to be processed in the
server&#39;s fax queue.</p><p><b>dwErrorEvents:</b> A <b>DWORD</b> that indicates
the number of error entries added to the system event log since the last time
the fax server was started.</p><p><b>dwWarningEvents:</b> A <b>DWORD</b> that indicates
the number of warning entries added to the system event log since the last time
the fax server was started.</p><p><b>dwInformationEvents:</b> A <b>DWORD</b> that
indicates the number of information entries added to the system event log since
the last time the fax server was started.</p></div>