<div class="content"><p>The <b>MIB_IPADDRTABLE</b> structure contains a table of
IPv4 address entries. This structure is used in <b>MIB_OPAQUE_INFO</b> (section
<a href="169e435d-a975-4c1c-bf41-55fd2bd76125" data-linktype="relative-path">2.2.1.2.52</a>) structure.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwNumEntries</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">table
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">...</p>
  </td>
 </tr>
</tbody></table><p><b>dwNumEntries (4 bytes): </b>The number of IPv4
address entries in the table.</p><p><b>table (variable): </b>A pointer to a table of IPv4
address entries implemented as an array of <a href="3dec2a67-bfd3-4a64-9e82-d1a51e86d844" data-linktype="relative-path"><b>MIB_IPADDRROW (section</b></a><span> </span>2.2.1.2.32) structures. </p></div>