<div class="content"><p> </p><p>This enumeration is used to represent specific address
types. As specified in the following descriptions, these address types can
change dynamically.</p><dl>
<dd>
<div><pre> typedef  enum _tag_FW_ADDRESS_KEYWORD
 {
   FW_ADDRESS_KEYWORD_NONE = 0x0000,
   FW_ADDRESS_KEYWORD_LOCAL_SUBNET = 0x0001,
   FW_ADDRESS_KEYWORD_DNS = 0x0002,
   FW_ADDRESS_KEYWORD_DHCP = 0x0004,
   FW_ADDRESS_KEYWORD_WINS = 0x0008,
   FW_ADDRESS_KEYWORD_DEFAULT_GATEWAY = 0x0010,
   FW_ADDRESS_KEYWORD_INTRANET = 0x0020,
   FW_ADDRESS_KEYWORD_INTERNET = 0x0040,
   FW_ADDRESS_KEYWORD_PLAYTO_RENDERERS = 0x0080,
   FW_ADDRESS_KEYWORD_REMOTE_INTRANET = 0x0100,
   FW_ADDRESS_KEYWORD_CAPTIVE_PORTAL = 0x0200,
   FW_ADDRESS_KEYWORD_MAX = 0x0400,
   FW_ADDRESS_KEYWORD_MAX_V2_10 = 0x0020,
   FW_ADDRESS_KEYWORD_MAX_V2_29 = 0x0200,
 } FW_ADDRESS_KEYWORD;
</pre></div>
</dd></dl><p><b>FW_ADDRESS_KEYWORD_NONE:</b>  Specifies that no
specific keyword is used.</p><p><b>FW_ADDRESS_KEYWORD_LOCAL_SUBNET:</b>  Represents
the collection of addresses that are currently within the local subnet of the
computer.</p><p><b>FW_ADDRESS_KEYWORD_DNS:</b>  Represents the
collection of addresses of the current DNS servers.</p><p><b>FW_ADDRESS_KEYWORD_DHCP:</b>  Represents the
collection of addresses of the current DHCP servers.</p><p><b>FW_ADDRESS_KEYWORD_WINS:</b>  Represents the
collection of addresses of the current WINS servers.</p><p><b>FW_ADDRESS_KEYWORD_DEFAULT_GATEWAY:</b> 
Represents the collection of addresses of the current gateway servers.</p><p><b>FW_ADDRESS_KEYWORD_INTRANET:</b>  Represents the
collection of addresses that are currently within the local intranet of the
computer. For schema versions 0x0200, 0x0201, and 0x020A, this value is invalid
and MUST NOT be used.</p><p><b>FW_ADDRESS_KEYWORD_INTERNET:</b>  Represents the
collection of addresses that are currently not within the local intranet or
remote intranet of the computer. For schema versions 0x0200, 0x0201, and
0x020A, this value is invalid and MUST NOT be used.</p><p><b>FW_ADDRESS_KEYWORD_PLAYTO_RENDERERS:</b> 
Represents the collection of addresses of the current Digital Media Renderer
devices as defined in <span><a href="../ms-dlnhnd/a12b022a-b793-46b2-aaa9-6100611b5038" data-linktype="relative-path">[MS-DLNHND]</a></span>
section <span><a href="../ms-dlnhnd/156db3e1-7df7-49bd-a317-65e6b78fd5c2" data-linktype="relative-path">3.3</a></span>.
For schema versions 0x0200, 0x0201, and 0x020A, this value is invalid and MUST
NOT be used.</p><p><b>FW_ADDRESS_KEYWORD_REMOTE_INTRANET:</b> 
Represents the collection of addresses that are currently within the remote
intranet of the computer. For schema versions 0x0200, 0x0201, and 0x020A, this
value is invalid and MUST NOT be used. </p><p><b>FW_ADDRESS_KEYWORD_CAPTIVE_PORTAL:</b>  Represents
the collection of addresses of the current captive portal. For schema versions
0x021D and earlier, this value is invalid and MUST NOT be used.</p><p><b>FW_ADDRESS_KEYWORD_MAX:</b>  This value and values
that exceed this value are not valid and MUST NOT be used. It is defined for
simplicity in writing <span><a href="d891304d-92d8-4f9f-9e60-a1f02b28ae30#gt_73177eec-4092-420f-92c5-60b2478df824" data-linktype="relative-path">IDL</a></span> definitions and
code. This symbolic constant has a value of 0x0400.</p><p><b>FW_ADDRESS_KEYWORD_MAX_V2_10:</b>  This value and
values that exceed this value are not valid and MUST NOT be used by servers and
clients with schema version 0x020A and earlier. It is defined for simplicity in
writing IDL definitions and code. This symbolic constant has a value of 0x0020.
</p><p><b>FW_ADDRESS_KEYWORD_MAX_V2_29:</b>  This value and
values that exceed this value are not valid and MUST NOT be used by servers and
clients with schema version 0x021D and earlier. It is defined for simplicity in
writing IDL definitions and code. This symbolic constant has a value of 0x0200.</p></div>