<div class="content"><p>The <b>_DRIVER_INFO_3</b> structure specifies <a href="831cd729-be7c-451e-b729-bd8d84ce4d24#gt_1a48eebd-e72c-494d-b8cb-84dfb7bc3b65" data-linktype="relative-path">printer driver</a> information.<a id="Appendix_A_Target_103"></a><a aria-label="Product behavior note 103" href="e81cbc09-ab05-4a32-ae4a-8ec57b436c43#Appendix_A_103" data-linktype="relative-path">&lt;103&gt;</a> It is a custom-<a href="831cd729-be7c-451e-b729-bd8d84ce4d24#gt_37e89d91-2800-49d1-9d17-45ebe167ad87" data-linktype="relative-path">marshaled</a> form of the <b>RPC_DRIVER_INFO_3</b>
(section <a href="b4d3b5f3-c631-4fc3-9348-4c983590a0d8" data-linktype="relative-path">2.2.1.5.3)</a>
structure.<span> </span></p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p>Fixed_Portion
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>Variable_Data
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
</tbody></table><p><b>Fixed_Portion (variable): </b>An array of one or
more groups of fixed-size fields, which are defined as follows.</p><dl>
<dd>
<table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p>cVersion</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>NameOffset</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>EnvironmentOffset</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>DriverPathOffset</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>DataFileOffset</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>ConfigFileOffset</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>HelpFileOffset</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>DependentFilesOffset</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>MonitorNameOffset</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>DefaultDataTypeOffset</p>
  </td>
 </tr>
</tbody></table>
</dd>
<dd>
<p><b>cVersion (4 bytes):</b> A
DWORD that has an implementation-specific value that identifies the driver
version and the operating system version for which the printer driver was
written, as specified in section <a href="4464eaf0-f34f-40d5-b970-736437a21913" data-linktype="relative-path">2.2.1.3.1</a>.</p>
</dd>
<dd>
<p><b>NameOffset (4 bytes):</b>
A 32-bit unsigned integer that specifies the number of bytes from the start of
the structure to the <b>NameArray</b> member.</p>
</dd>
<dd>
<p><b>EnvironmentOffset (4
bytes):</b> An unsigned integer that specifies the number of bytes from the
start of the structure to the start of the <b>EnvironmentArray</b> member. </p>
</dd>
<dd>
<p><b>DriverPathOffset (4
bytes):</b> An unsigned integer that specifies the number of bytes from the
start of the structure to the start of the <b>DriverPathArray</b> member. </p>
</dd>
<dd>
<p><b>DataFileOffset (4 bytes):</b>
An unsigned integer that specifies the number of bytes from the start of the
structure to the start of the <b>DataFileArray</b> member. </p>
</dd>
<dd>
<p><b>ConfigFileOffset (4
bytes):</b> An unsigned integer that specifies the number of bytes from the
start of the structure to the start of the <b>ConfigFileArray</b> member. </p>
</dd>
<dd>
<p><b>HelpFileOffset (4 bytes):</b>
An unsigned integer that specifies the number of bytes from the start of the
structure to the start of the <b>HelpFileArray</b> member. </p>
</dd>
<dd>
<p><b>DependentFilesOffset (4
bytes):</b> An unsigned integer that specifies the number of bytes from the
start of the structure to the start of the <b>DependentFilesArray</b> member. </p>
</dd>
<dd>
<p><b>MonitorNameOffset (4
bytes):</b> An unsigned integer that specifies the number of bytes from the
start of the structure to the start of the <b>MonitorNameArray</b> member. </p>
</dd>
<dd>
<p><b>DefaultDataTypeOffset (4
bytes):</b> An unsigned integer that specifies the number of bytes from the
start of the structure to the start of the <b>DefaultDataTypeArray</b> member.</p>
</dd></dl><p><b>Variable_Data (variable):</b> An array of zero or
more groups of optional, variable-size fields, which are defined as follows.</p><dl>
<dd>
<table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p>DefaultDataTypeArray
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>MonitorNameArray
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>DependentFilesArray
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>HelpFileArray
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>ConfigFileArray
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>DataFileArray
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>DriverPathArray
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>EnvironmentArray
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>NameArray
  (variable)</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p>...</p>
  </td>
 </tr>
</tbody></table>
</dd>
<dd>
<p><b>DefaultDataTypeArray
(variable):</b> A string that specifies the default data type of print jobs
created by the driver. The location of this buffer is determined by the value
of the <b>DefaultDataTypeOffset</b> member. </p>
</dd>
<dd>
<p><b>MonitorNameArray
(variable):</b> A string that specifies a language monitor. The location of
this buffer is determined by the value of the <b>MonitorNameOffset</b> member. </p>
</dd>
<dd>
<p><b>DependentFilesArray
(variable):</b> A multisz that specifies the names of the files that the
printer driver is dependent on. The location of this buffer is determined by
the value of the <b>DependentFilesOffset</b> member. </p>
</dd>
<dd>
<p><b>HelpFileArray (variable):</b>
A string that specifies a file name or a full path and file name for the
printer driver help file. The location of this buffer is determined by the
value of the <b>HelpFileOffset</b> member. </p>
</dd>
<dd>
<p><b>ConfigFileArray
(variable):</b> A string that specifies a file name or a full path and file
name for the printer driver configuration module. The location of this buffer
is determined by the value of the <b>ConfigFileOffset</b> member. </p>
</dd>
<dd>
<p><b>DataFileArray (variable):</b>
A string that specifies a file name or a full path and file name for the file
that contains printer driver data. The location of this buffer is determined by
the value of the <b>DataFileOffset</b> member. </p>
</dd>
<dd>
<p><b>DriverPathArray
(variable):</b> A string that specifies a file name or full path and file name
for the file that contains the printer driver. The location of this buffer is
determined by the value of the <b>DependentFilesOffset</b> member. </p>
</dd>
<dd>
<p><b>EnvironmentArray
(variable):</b> A string that specifies the environment that the printer driver
supports. The location of this buffer is determined by the value of the <b>EnvironmentOffset</b>
member. </p>
</dd>
<dd>
<p><b>NameArray (variable):</b>
This member MUST contain a string that specifies the print processor name. The
location of this buffer is determined by the value of the <b>NameOffset</b>
member. For rules governing print processor names, see section <a href="807e0bdd-21a5-4a72-9a6a-1a7fb1b08a8e" data-linktype="relative-path">2.2.4.11</a>.</p>
</dd></dl></div>