<div class="content"><p>The <b>RASMAN_USAGE</b> enumerates the usage for a port. It
can be any combination of the following values.</p><dl>
<dd>
<div><pre> typedef enum _RASMAN_USAGE
 {
   CALL_NONE = 0x00,
   CALL_IN = 0x01,
   CALL_OUT = 0x02,
   CALL_ROUTER = 0x04,
   CALL_LOGON = 0x08,
   CALL_OUT_ONLY = 0x10,
   CALL_IN_ONLY = 0x20,
   CALL_OUTBOUND_ROUTER = 0x40
 } RASMAN_USAGE;
</pre></div>
</dd></dl><p><b>CALL_NONE: </b>Port is not configured for any
usage.</p><p><b>CALL_IN: </b>Port is configured for incoming
connection requests.</p><p><b>CALL_OUT: </b>Port is configured for outgoing
connection requests</p><p><b>CALL_ROUTER: </b>Port is configured for
demand-dial connection requests.</p><p><b>CALL_LOGON: </b>Port is configured for connection
during logon.</p><p><b>CALL_OUT_ONLY: </b>Port is configured only for
outgoing connection requests.</p><p><b>CALL_IN_ONLY: </b>Port is configured only for
incoming connection requests.</p><p><b>CALL_OUTBOUND_ROUTER: </b>Port is configured for
outgoing demand-dial connection requests.</p></div>