<div class="content"><p>The LINE_REPLY packet is sent to report the results of a
function call that completed asynchronously.</p><table>
 <tbody><tr>
  <th><p><br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>1<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>2<br/>0</p></th>
  <th><p><br/>1</p></th>
  <th><p><br/>2</p></th>
  <th><p><br/>3</p></th>
  <th><p><br/>4</p></th>
  <th><p><br/>5</p></th>
  <th><p><br/>6</p></th>
  <th><p><br/>7</p></th>
  <th><p><br/>8</p></th>
  <th><p><br/>9</p></th>
  <th><p>3<br/>0</p></th>
  <th><p><br/>1</p></th>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">TotalSize</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">InitContext</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">fnPostProcessProcHandle</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">hDevice</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Msg</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">OpenContext</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwRemoteRequestID</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">dwParam2</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved1</p>
  </td>
 </tr>
 <tr>
  <td colspan="32">
  <p align="center">Reserved2</p>
  </td>
 </tr>
</tbody></table><p><b>TotalSize (4 bytes): </b>An unsigned 32-bit
integer. The total size of the asynchronous event packet.</p><p><b>InitContext (4 bytes): </b>An unsigned 32-bit
integer. The opaque, client-specified session value that MUST be equal to the
InitContext value that is specified in the original scoping of the line <a href="9d8eb7cd-3245-4e44-97e0-42f7b89c9424" data-linktype="relative-path">Initialize</a> request.</p><p><b>fnPostProcessProcHandle (4 bytes): </b>An unsigned
32-bit integer. The opaque, client-specified value that MUST be equal to the
lpContext value in the original request.</p><p><b>hDevice (4 bytes): </b>An unsigned 32-bit integer.
The handle to the call or line device that is associated with the asynchronous
event.</p><p><b>Msg (4 bytes): </b>An unsigned 32-bit integer. The
packet type; MUST be set to 0x0000000C (LINE_REPLY).</p><p><b>OpenContext (4 bytes): </b>An unsigned 32-bit
integer. The opaque, client-specified context value that MUST be equal to the OpenContext
value that is specified in the original scoping of the line <a href="2759c744-e040-4c5d-b4b5-215d391f0490" data-linktype="relative-path">Open</a> request.</p><dl>
<dd>
<p>This information MUST be passed back to the
application with each completion and event that is associated with the handle
of the line or call on the line. This field is not interpreted by TAPI.</p>
</dd></dl><p><b>dwRemoteRequestID (4 bytes): </b>An unsigned
32-bit integer. The <a href="489de77f-16d8-4c4f-939a-f795e8b42893#gt_60e0e1fa-66fe-41e1-b5e3-ceab97e53506" data-linktype="relative-path">client</a>
ID for the request value.</p><p><b>dwParam2 (4 bytes): </b>An unsigned 32-bit
integer. Indicates success or error. A zero indicates success; a negative
number indicates an error.</p><p><b>Reserved1 (4 bytes): </b>An unsigned 32-bit
integer. This MUST be ignored on receipt and can be any value.  </p><p><b>Reserved2 (4 bytes): </b>An unsigned 32-bit
integer. This MUST be ignored on receipt and can be any value.  </p></div>